**N1-MAF1498-DG Receiver firmware upgrade instructions Version1.0**

Step1: Double click on the file ”**MAF1498-dongle-2.23**” on the computer to open it. (If antivirus software is installed on your computer, please temporarily close the antivirus software before opening this file.After the firmware upgrade is completed, reopen the antivirus software.)

Step2: Please hold down the button on the receiver and connect it to the computer through the USB port of the receiver. Wait for the firmware upgrade to be recognized successfully, then release the button.

Step3: Wait a few seconds, Download progress Display 100%, the receiver firmware upgrade completed.